|  |  |
| --- | --- |
| **Colour** | Black/Red/Green |
| **Hardness** | 40 +/-5 ShoreA |
| **Tensile Strength** | 18MPA |
| **Elongation** | 600% |
| **Temperature Range** | -20°C to 60°C |
| **Surface** | Smooth |
| **Density** | 1.05g/cm³ |



**Natural Rubber IRHD40/45**

* Excellent abrasion resistance
* Also known as Gum Rubber or Wear Rubber.
* Conveyor Skirting Rubber